	#
	Description
	Qty
	UoM
	Price per Unit, $
	Total Price, $

	1
	1.000, Pipe, A333-6, SMLS, Sch XXS, PE
	12
	M
	
	

	2
	1.000, Pipe, A333-6, SMLS, Sch XXS, PE
	6
	M
	
	

	3
	PPPCH90D6Z0M 1.000, Pipe, A333-6, SMLS, Sch 160, PE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 160 Seamless Plain End Per
	6
	M
	
	

	4
	1.000, PIPE, B423-825, SMLS, SCH 40S, PE
	6
	M
	
	

	5
	PPPCH90N7000 2.000, Pipe, A333-6, SMLS, 0.500" WT, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6, 0.500 Inch Wall Thk., Seamless,
	12
	M
	
	

	6
	PPPCH9087000 2.000, Pipe, A333-6, 2", SMLS, Sch 80, PE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 80 Seamless Bevelled  B
	12
	M
	
	

	7
	PPPCH9057002 3.000, Pipe, 3", A333-6, SMLS, StdWt, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Standard Weight Seamless Bevelle
	12
	M
	
	

	8
	PPPCZA0G6V02 3.000, Pipe, B423-825, SMLS, Sch40S, BBE, Pipe Nickel Alloy Per ASTM B423  UNS NO8825 Cold Worked Annealed Schedule
	12
	M
	
	

	9
	PPPCH90Z8Q04 6.000, Pipe, A333-6, SMLS 1.063" W, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Seamless, 1.063" Wall, Bevelled  B
	48
	M
	
	

	10
	PPPCX80G6V04 6.000, Pipe, A312TP304*, SMLS, Sch40S, BBE, Pipe Dual Grade Stainless Steel Per ASTM A312 Grade TP304/304L Schedule
	12
	M
	
	

	11
	PPPCH9057004 6.000, Pipe, A333-6, SMLS, StdWt, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Standard Weight Seamless Bevelled  B
	12
	M
	
	

	12
	PPPCH90X7005 8.000, Pipe, A333-6, SMLS, 1.375" WT, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6, 1.375 Inch Wall Thk.,Seamless,
	14.4
	M
	
	

	13
	PPPCH9057005 8.000, Pipe, A333-6, SMLS, StdWt, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Standard Weight Seamless Bevelled  B
	15.6
	M
	
	

	14
	PPPCH90Z8R0610.000, Pipe, A333-6, SMLS, 1.625" WT, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Seamless, 1.625" Wall Thk., Beve
	12
	M
	
	

	15
	PPPCH905700610.000, Pipe, A333-6, SMLS, StdWt, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Standard Weight Seamless Bevelled  B
	12
	M
	
	

	16
	PPPCH9067006 10.000, Pipe, 10", A333-6, SMLS, Sch 60, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 60 Seamless Bevelled
	12
	M
	
	

	17
	PPPCH906700712.000, Pipe, A333-6, SMLS, Sch 60, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 60 Seamless Bevelled Both
	12
	M
	
	

	18
	PPPCH904700712.000, Pipe, A333-6, SMLS, Sch 40, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 40 Seamless Bevelled Both
	12
	M
	
	

	19
	PPPCH905700712.000, Pipe, A333-6, SMLS, StdWt, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Standard Weight Seamless Bevelled  B
	12
	M
	
	

	20
	PPPCH905700814.000, Pipe, A333-6, SMLS, StdWt, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Standard Weight Seamless Bevelled  B
	12
	M
	
	

	21
	PPPCH908700916.000, Pipe, A333-6, SMLS, Sch 80, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 80 Seamless Bevelled Both
	12
	M
	
	

	22
	PPPCH90A700916.000, Pipe, A333-6, SMLS, Sch 100, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 100 Seamless Bevelled Bot
	12
	M
	
	

	23
	PPPCJF0X7F0F30.000, Pipe, A671-CC 60-22, EFW, 1.375" WT, BBE, Pipe Carbon Steel Per ASTM A671 Grade CC60 Class 22 1.375 Inch Wal
	12
	M
	
	

	24
	PPPCH9087005 8.000 Pipe, A333-6, SMLS, Sch 80, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 80 Seamless Bevelled Both Ends Per ANSI B36.10 Material Shall Meet the Requirements of NACE MR0175 To be
Supplied in Double Random Lengths
	2.4
	M
	
	

	25
	PPPCH9067005 8.000, Pipe, A333-6, SMLS, Sch 60, BBE, Pipe Carbon Steel Per ASTM A333 Grade 6 Schedule 60 Seamless Bevelled Both
 Ends Per ANSI B36.10 Material Shall Meet the Requirements of NACE MR0175 To be Supplied in Double Random Lengths
	2.7
	M
	
	

	 
	 
	 
	
	

	26
	PFNPX80G7C04 0.750, Nipple, PBE, A312-TP304/304L, Sch 40S, 100 mm, Nipple Dual Grade Stainless Steel Per ASTM A312 Grade TP304/3
	2
	EA
	
	

	27
	PFNPH9087N04 0.750, Nipple, PBE, A333-6, Sch 80, 100 mm, Nipple Carbon Steel Per ASTM A333 Grade 6 Schedule 80 Plain Both Ends
	2
	EA
	
	

	28
	PFNPH9087P04 0.750, Nipple, PBE, A333-6, Sch 80, 200 mm, Nipple Carbon Steel Per ASTM A333 Grade 6 Schedule 80 Plain Both Ends
	2
	EA
	
	

	29
	PFNPH90D7G04 0.750, Nipple, BE, A333-6, Sch 160, 100 mm, Nipple Carbon Steel Per ASTM A333 Grade 6, Schedule 160, Beveled Ends,
	2
	EA
	
	

	30
	PFNPH90D7G05 1.000, Nipple, BE, A333-6, Sch 160, 100 mm, Nipple Carbon Steel Per ASTM A333 Grade 6, Schedule 160, Beveled Ends,
	4
	EA
	
	

	31
	PFNPH9097G05 1.000, Nipple, BE, A333-6, XXS, 100 mm, Nipple Carbon Steel Per ASTM A333 Grade 6, Double Extra Strong, Beveled End
	2
	EA
	
	

	32
	2.000, NIPPLE, TBEM, A333-6, SCH 80, 100 MM, GALV
	3
	M
	
	

	 
	 
	 
	
	

	33
	PFCNHE0D8B02 1.000, El, 90Deg, 1", LR, BW, A420-WPL6, Sch 160, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Schedule 160 Buttweld
	4
	EA
	
	

	34
	PFCVHE0N7P08 2.000 1.000, RedTee, BW, A420-WPL6, 0.500" WT x Sch XXS, Tee - Reducing Carbon Steel Per ASTM A420 Grade WPL6 0.500
	4
	EA
	
	

	35
	PFCNHE0NEK04 2.000, El, 2", 90 Deg, LR, BW, A420-WPL6, 0.500" WT, Elbow Carbon Steel Per ASTM A420 Grade WPL6 0.500 Inch Wall Bu
	4
	EA
	
	

	36
	PFCNZC0G8B0G 3.000, El, 90Deg, LR, BW, B366-825, Sch40S, Elbow Nickel Alloy Per ASTM B366 Grade WPNICMCS UNS NO8825 Schedule 40S
	2
	EA
	
	

	37
	PFCNVA0G8B0K 6.000, El, 90 Deg, LR, BW,A403-WP304/304L-S, Sch 40S, Elbow Dual Grade Stainless Steel Per ASTM A403 Grade WP304/30
	4
	EA
	
	

	38
	PFCTVA0G4Y0K 6.000, Te, BW, A403WP304/304L-S, Sch40S, Tee - Equal Dual Grade Stainless Steel Per ASTM A403 Grade WP304/304L-S Sc
	2
	EA
	
	

	39
	PFCTHE0Z6E0K 6.000, Tee, BW, A420-WPL6, 1.063" WT, Tee - Equal Carbon Steel Per ASTM A420 Grade WPL6 1.063 Inch Wall, Buttweld
	3
	EA
	
	

	40
	PFCNHE058B0K 6.000, El, 90Deg, LR, BW, A420-WPL6, StdWt, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Standard Weight Buttweld En
	2
	EA
	
	

	41
	PFCNHE058B0L 8.000, El, 90Deg, LR, BW, A420-WPL6, StdWt, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Standard Weight Buttweld En
	2
	EA
	
	

	42
	PFCNHE058B0M10.000, El, 90Deg, LR, BW, A420-WPL6, StdWt, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Standard Weight Buttweld En
	7
	EA
	
	

	43
	PFCNHE068B0M10.000, El, 90Deg, LR, BW, A420-WPL6, Sch 60, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Schedule 60 Buttweld End 9
	10
	EA
	
	

	44
	PFCNHE068C0M10.000, El, 45Deg, LR, BW, A420-WPL6, Sch 60, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Schedule 60 Buttweld End 4
	4
	EA
	
	

	45
	PFCNHE0ZER0M10.000, El, 90 Deg, LR, BW, A420-WPL6, 1.625" WT, Elbow Carbon Steel Per ASTM A420 Grade WPL6 1.625 Inch Wall, Buttw
	3
	EA
	
	

	46
	PFCNHE048B0N 12.000, El, 90Deg, 12", LR, BW, A420-WPL6, Sch 40, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Schedule 40 Buttweld
	4
	EA
	
	

	47
	PFCNHE058B0N12.000, El, 90Deg, LR, BW, A420-WPL6, StdWt, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Standard Weight Buttweld En
	2
	EA
	
	

	48
	PFCNHE088B0Q16.000, El, 90Deg, LR, BW, A420-WPL6, Sch 80, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Schedule 80 Buttweld End 9
	5
	EA
	
	

	49
	PFCNHE0A8B0Q16.000, El, 90Deg, LR, BW, A420-WPL6, Sch 100, Elbow Carbon Steel Per ASTM A420 Grade WPL6 Schedule 100 Buttweld End
	2
	EA
	
	

	50
	PFCSHF0XAF3P30.00024.000, RedEcc, BW, A420-WPL6W, 1.375" WT x Sch 80, Reducer - Eccentric Carbon Steel Per ASTM A420 Grade WPL6-
	3
	EA
	
	

	51
	PFCSHE055R1H14.00010.000, RedEcc, BW, A420-WPL6, StdWt, Reducer - Eccentric Carbon Steel Per ASTM A420 Grade WPL6 Standard Weigh
	2
	EA
	
	

	52
	2.000 0.750, REDCON, BW, A420-WPL6, SCH 80
	3
	EA
	
	

	53
	PFCVHE056R2K 3.000 2.000, RedTe, BW, A420-WPL6, StdWt x Sch 80, Tee - Reducing Carbon Steel Per ASTM A420 Grade WPL6 Standard We
	3
	EA
	
	

	54
	PFCVZC0G6G29 4.000 3.000, RedTe, BW, B366-825, Sch40S, Tee - Reducing Nickel Alloy Per ASTM B366 Grade WPNICMCS UNS NO8825 Sched
	2
	EA
	
	

	55
	PFCVHE056G1R10.000 6.000, RedTe, BW, A420-WPL6, StdWt, Tee - Reducing Carbon Steel Per ASTM A420 Grade WPL6 Standard Weight  But
	2
	EA
	
	

	56
	PFCVHE056G1G14.00012.000, RedTe, BW, A420-WPL6, StdWt, Tee - Reducing Carbon Steel Per ASTM A420 Grade WPL6 Standard Weight  But
	3
	EA
	
	

	57
	24.000 X 16.000, REDTEE, BW, A420-WPL6, SCH 100
	2
	EA
	
	

	58
	PFCVHF0X9Q5M30.00016.000, RedTee, BW, A420-WPL6W, 1.375" WT x Sch 80, Tee - Reducing Carbon Steel Per ASTM A420 Grade WPL6-W 1.3
	3
	EA
	
	

	 
	 
	 
	
	

	59
	PFLWHB083606 2.000 0.750, Weldolet, A350LF2, Sch 80, Weldolet, Carbon Steel per ASTM A350 Grade LF2, Schedule 80, Per MSS SP 97,
	2
	EA
	
	

	60
	3.000 X 1.000, WELDOLET, B564-825, SCH 40S
	2
	EA
	
	

	61
	6.000 X 0.750, WELDOLET, A350-LF2, STDWT X SCH 80
	2
	EA
	
	

	62
	6.000 X 0.750, WELDOLET, A182-F304/304L, SCH 40S
	2
	EA
	
	

	63
	PFLWHB0541NN 6.000 1.000, Weldolet, A350LF2, StdWt x Sch 160, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Standard Weight Sche
	2
	EA
	
	

	64
	PFLWHB0Z4RNN 6.000 1.000, Weldolet, A350-LF2, 1.063" WT x Sch XXS, Weldolet Carbon Steel Per ASTM A350 Grade LF2 1.063 Inch Wall
	6
	EA
	
	

	65
	PFLWHB0Z448F 6.000 2.000, Weldolet, 6IN X 2IN, A350-LF2, 1.063" WT x 0.500" WT, Weldolet Carbon Steel Per ASTM A350 Grade LF2 1.
	2
	EA
	
	

	66
	PFLWHB05418L 8.000 0.750, Weldolet, A350LF2, StdWt x Sch 160, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Standard Weigth Sche
	2
	EA
	
	

	67
	PFLWHB0Z4SNP 8.000 1.000, Weldolet, A350-LF2, 1.375" WT x Sch XXS, Weldolet Carbon Steel Per ASTM A350 Grade LF2 1.375 Inch Wall
	11
	EA
	
	

	68
	PFLWHB0541NQ10.000 1.000, Weldolet, A350LF2, StdWt x Sch 160, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Standard Weight Sche
	4
	EA
	
	

	69
	PFLWHB063CNQ 10.0 1.0, Weldolet, A350LF2, Sch 60 x Sch XXS, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Schedule 60 Double Ext
	7
	EA
	
	

	70
	PFLWHB0Z4TNQ10.000 1.000, Weldolet, A350-LF2, 1.625" WT x Sch XXS, Weldolet Carbon Steel Per ASTM A350 Grade LF2 1.625 Inch Wall
	4
	EA
	
	

	71
	PFLWHB053D8X10.000 2.000, Weldolet, A350LF2, StdWt x Sch 80, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Standard Weight Sched
	2
	EA
	
	

	72
	PFLWHB053D9512.000 2.000, Weldolet, A350LF2, StdWt x Sch 80, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Standard Weight Sched
	2
	EA
	
	

	73
	PFLWHB0836NT16.000 1.000, Weldolet, A350-LF2, Sch 80 x Sch 160, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Schedule 80  Sched
	3
	EA
	
	

	74
	PFLWHB0A3CNT 16.0 1.0, Weldolet, A350-LF2, Sch 100 x Sch XXS, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Schedule 100 Duoble
	2
	EA
	
	

	75
	PFLWHB073FGU42.000 8.000, Weldolet, A350LF2, Sch XS x StdWt, Weldolet Carbon Steel Per ASTM A350 Grade LF2 Extra Strong Standard
	2
	EA
	
	

	 
	 
	 
	
	

	76
	0.750, FlgWN, A350-LF2, CL150, Sch80, RF, B16.5
	3
	EA
	
	

	77
	0.750, FlgWN, A350-LF2, CL150, Sch80, RF, B16.5
	2
	EA
	
	

	78
	0.750 X 0.750, FLGWN, A182-F304/304L, CL 300, SCH 40S, RF, B16.5
	2
	EA
	
	

	79
	PFFB04302V01 0.750, FlgBlnd, A182-F304/304L,CL 300, RF, B16.5, Flange - Blind Dual Grade Stainless Steel Per ASTM A182 Grade  F3
	2
	EA
	
	

	80
	PFFWHB1D1302 1.000, FlgWN, A350LF2, CL150, Sch 160, RF, B16.5, 1" Weld Neck Flange, Carbon Steel Per ASTM A350 Gr. LF2, ASME Cla
	2
	EA
	
	

	81
	PFFWHBJ90502 1.000, FlgWN, A350LF2, CL2500, XXS, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	20
	EA
	
	

	82
	1.000, FLGWN, B564-825, CL 150, SCH 40S, RF, B16.5
	2
	EA
	
	

	83
	PFFWHB391302 1.000, FlgWN, A350 LF2, CL300, Sch XXS, RF, B16.5, 1" Weld Neck Flange, Carbon Steel Per ASTM A350 Gr. LF2, ASME  C
	4
	EA
	
	

	84
	PFFWHB6D0502 1.000, FlgWN, A350-LF2, CL 600, Sch 160, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME
	3
	EA
	
	

	85
	PFFWHB690X02 1.000, FlgWN, A350-LF2, CL 600, Sch XXS, RTJ, B16.5, 1 " Weld Neck Flange, Carbon Steel Per ASTM A350 Gr. LF2, ASME
	2
	EA
	
	

	86
	PFFWHBJ90502 1.000, FlgWN, A350LF2, CL2500, XXS, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	4
	EA
	
	

	87
	PFFWHB3D1302 1.000, FlgWN, A350LF2, CL300, Sch 160, RF, B16.5, 1" Weld Neck Flange, Carbon Steel Per ASTM A350 Gr. LF2, ASME Cla
	4
	EA
	
	

	88
	PFFBHBJ00P02 1.000, FlgBlnd, A350LF2, CL2500, RTJ, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 2500  R
	20
	EA
	
	

	89
	PFFBHBJ00P05 2.000, FlgBlnd, A350LF2, CL2500, RTJ, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 2500  R
	2
	EA
	
	

	90
	PFFWHBJN0505 2.000, FlgWN, A350-LF2, CL 2500, 0.500" WT, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASM
	11
	EA
	
	

	91
	PFXAKZJ03G04 2.000, Blnd-Spec, FRTJ, A516-70, CL2500, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 2500  Fem
	4
	EA
	
	

	92
	PFFWHB182W05 2.000, FlgWN, A350LF2, CL150, Sch 80, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	6
	EA
	
	

	93
	PFFTHB101N05 2.000, FlgThd, A350LF2, CL150, FF, B16.5, Flange- Threaded Carbon Steel Per ASTM A350 Grade LF2 ASME Class 150 Flat
	4
	EA
	
	

	94
	3.000, FLGWN, B564-825, CL 150, SCH 40S, RF, B16.5
	5
	EA
	
	

	95
	PFFWHB152W06 3.000, FlgWN, A350LF2, CL150, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	5
	EA
	
	

	96
	4.000, FLGWN, B564-825, CL 150, SCH 40S, RF, B16.5
	5
	EA
	
	

	97
	PFFWHB152W0A 6.000, FlgWN, A350LF2, CL150, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	9
	EA
	
	

	98
	PFFB04302V0A 6.000, FlgBlnd, A182-F304/304L,CL 300, RF, B16.5, Flange - Blind Dual Grade Stainless Steel Per ASTM A182 Grade F30
	2
	EA
	
	

	99
	PFFBHBJ00P0A 6.000, FlgBlnd, A350LF2, CL2500, RTJ, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 2500  R
	2
	EA
	
	

	100
	PFFWHBJZ370A 6.000, FlgWN, A350-LF2, CL 2500, 1.063" WT, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASM
	21
	EA
	
	

	101
	PFFW043G2W0A 6.000, FlgWN, A182-F304/304L, CL 300, Sch 40S, RF, B16.5, Flange - Weld Neck Dual Grade Stainless Steel Per ASTM A1
	7
	EA
	
	

	102
	PFXAKZJ03G0K 6.000, Blnd-Spec, FRTJ, A516-70, CL2500, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 2500 Fema
	6
	EA
	
	

	103
	PFXA0C303L0K 6.000, Blnd-Spec, RF, A240-304*, CL300, Blind - Spectacle Dual Grade Stainless Steel Per ASTM A240 Grade 304/304L A
	2
	EA
	
	

	104
	PFFWHB152W0B 8.000, FlgWN, A350LF2, CL150, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	7
	EA
	
	

	105
	PFFWHBJX050B 8.000, FlgWN, A350-LF2, CL 2500, 1.375" WT, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASM
	33
	EA
	
	

	106
	PFXAKZJ03G0L 8.000, Blnd-Spec, FRTJ, A516-70, CL2500, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 2500  Fem
	11
	EA
	
	

	107
	PFFWHB152W0C10.000, FlgWN, A350LF2, CL150, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	5
	EA
	
	

	108
	PFFWHB162W0C10.000, FlgWN, A350LF2, CL150, Sch 60, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	7
	EA
	
	

	109
	PFFWHB352W0C10.000, FlgWN, A350LF2, CL300, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	14
	EA
	
	

	110
	PFFWHB362W0C10.000, FlgWN, A350LF2, CL300, Sch 60, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	16
	EA
	
	

	111
	PFFWHBJZ380C10.000, FlgWN, A350-LF2, CL 2500, 1.625" WT, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASM
	10
	EA
	
	

	112
	PFFWHB152W0D12.000, FlgWN, A350LF2, CL150, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	5
	EA
	
	

	113
	PFFWHB342W0D12.000, FlgWN, A350LF2, CL300, Sch 40, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	10
	EA
	
	

	114
	PFFWHB142W0D12.000, FlgWN, A350LF2, CL150, Sch 40, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	7
	EA
	
	

	115
	PFFWHB362W0D12.000, FlgWN, A350LF2, CL300, Sch 60, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	4
	EA
	
	

	116
	PFFWHB352W0D12.000, FlgWN, A350LF2, CL300, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	2
	EA
	
	

	117
	PFFWHB152W0E14.000, FlgWN, A350LF2, CL150, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	5
	EA
	
	

	118
	PFFWHB352W0E14.000, FlgWN, A350LF2, CL300, StdWt, RF, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME Class
	2
	EA
	
	

	119
	PFFWHB68050F16.000, FlgWN, A350-LF2, CL 600, Sch 80, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME  C
	9
	EA
	
	

	120
	PFFWHB6A050F16.000, FlgWN, A350-LF2, CL 600, Sch 100, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME C
	5
	EA
	
	

	121
	PFFWHB68050K24.000, FlgWN, A350-LF2, CL 600, Sch 80, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME  C
	5
	EA
	
	

	122
	PFFWHB6A050K24.000, FlgWN, A350-LF2, CL 600, Sch 100, RTJ, B16.5, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 ASME
	3
	EA
	
	

	123
	PFFWHB6X3K0M30.000, FlgWN, A350-LF2, CL 600, 1.375" WT, RTJ, B16.47-A, Flange - Weld Neck Carbon Steel Per ASTM A350 Grade LF2 A
	5
	EA
	
	

	124
	PFFWHB1D1301 0.750, FlgWN, A350LF2, CL150, Sch160, RF, B16.5, 3/4" Weld Neck Flange, Carbon Steel Per ASTM A350 Gr. LF2, ASME Cl
	2
	EA
	
	

	125
	0.750, FlgWN, A350-LF2, CL150, Sch80, RF, B16.5
	2
	EA
	
	

	126
	PFFWHB3D1301 0.750, FlgWN, A350LF2, CL300, Sch 160, RF, B16.5, 3 / 4" Weld Neck Flange, Carbon Steel Per ASTM A350 Gr. LF2, ASME
	4
	EA
	
	

	127
	PFFBHB302V01 0.750, FlgBlnd, A350LF2, CL300, RF, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 300 Raise
	6
	EA
	
	

	128
	PFFBHB102V01 0.750, FlgBlnd, A350LF2, CL150, RF, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 150 Raise
	4
	EA
	
	

	129
	PFFBHB102V02 1.000, FlgBlnd, A350LF2, CL150, RF, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 150 Raise
	3
	EA
	
	

	130
	PFFBHB302V02 1.000, FlgBlnd, A350LF2, CL300, RF, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 300 Raise
	7
	EA
	
	

	131
	PFFBHB600P02 1.000, FlgBlnd, A350LF2, CL600, RTJ, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 600 Ring
	4
	EA
	
	

	132
	PFFBHBJ00P02 1.000, FlgBlnd, A350LF2, CL2500, RTJ, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 2500  R
	4
	EA
	
	

	133
	PFFBHB600P0K24.000, FlgBlnd, A350LF2, CL600, RTJ, B16.5, Flange - Blind Carbon Steel Per ASTM A350 Grade LF2 ASME Class 600 Ring
	2
	EA
	
	

	134
	PFXAKZ103B04 2.000, Blnd-Spec, RF, A516-70, CL150, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 150 Raised
	3
	EA
	
	

	135
	PFXAKZ103R04 2.000, Blnd-Spec, FF, A516-70, CL150, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 150 Flat Fac
	2
	EA
	
	

	136
	PFXAZD103L0G 3.000, Blnd-Spec, RF, B424-825, CL150, Blind - Spectacle Nickel Alloy Per ASTM B424 UNS NO8825 Annealed ASME Class
	2
	EA
	
	

	137
	PFXAKZ103B0K 6.000, Blnd-Spec, RF, A516-70, CL150, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 150 Raised
	3
	EA
	
	

	138
	PFXAKZ103B0L 8.000, Blnd-Spec, RF, A516-70, CL150, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 150 Raised
	2
	EA
	
	

	139
	PFXAKZ303B0M10.000, Blnd-Spec, RF, A516-70, CL300, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 300 Raised
	2
	EA
	
	

	140
	PFXAKZJ03G0M 10.000, Blnd-Spec, FRTJ, A516-70, CL2500, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 2500 Fem
	4
	EA
	
	

	141
	PFXAKZ103B0N12.000, Blnd-Spec, RF, A516-70, CL150, Blind - Spectacle Carbon Steel Per ASTM A516 Grade 70 ASME Class 150 Raised
	2
	EA
	
	

	142
	PFFKKZ603A0F16.000, Bld & Spcr, A516-70, CL 600, FRTJ, API 590, Flange - Blind and Spacer Carbon Steel Per ASTM A516 Grade 70 AS
	4
	EA
	
	

	143
	300-SP-14.000, KIT,FLANGE INSULATION: 14IN,CL300,RF, Data Sht KPO-00-PIP-DTS-00801
	1
	EA
	
	

	 
	 
	
	

	144
	PGGC2S300600 0.750, Gasket, SpWnd, 316-FG, 1/8"SS,CL 300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled  A
	3
	EA
	
	

	145
	PGGC2S100600 0.750, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	10
	EA
	
	

	146
	PGGC2S300600 0.750, Gasket, SpWnd, 316-FG, 1/8"SS,CL 300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled  A
	3
	EA
	
	

	147
	PGGC2S100602 1.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	3
	EA
	
	

	148
	PGGC2Z103W02 1.000, Gasket, SpWnd, 825/Grph, 1/8", CL 150, B16.20, Gasket Incoloy 825 Flexible Graphite Filled ASME Class 150  S
	3
	EA
	
	

	149
	PGGC2S300602 1.000, Gasket, SpWnd, 316-FG, 1/8"SS,CL 300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled  A
	14
	EA
	
	

	150
	PGGC1Y600A02 1.000, Gasket, OvlRng, Soft Iron, R16, CL 600, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  Cl
	5
	EA
	
	

	151
	PGGC1YJ00A02 1.000, Gasket, OvlRng, Soft Iron, R18, CL 2500, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  C
	7
	EA
	
	

	152
	PGGC1Y600A02 1.000, Gasket, OvlRng, Soft Iron, R16, CL 600, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  Cl
	3
	EA
	
	

	153
	PGGC1YJ00A02 1.000, Gasket, OvlRng, Soft Iron, R18, CL 2500, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  C
	40
	EA
	
	

	154
	PGGC1YJ00A04 2.000, Gasket, OvlRng, Soft Iron, R26, CL 2500, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  C
	22
	EA
	
	

	155
	PGGC2S100604 2.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	5
	EA
	
	

	156
	PGGC3Y100104 2.000, Gasket, FlatFF, Non AsbFib,1/16", CL 150, B16.21, B16.5, Gasket Compressed Non-Asbestos Fibre ASME Class 150
	4
	EA
	
	

	157
	PGGC2S100606 3.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	3
	EA
	
	

	158
	PGGC2Z103W06 3.000, Gasket, SpWnd, 825/Grph, 1/8", CL 150, B16.20, Gasket Incoloy 825 Flexible Graphite Filled ASME Class 150  S
	6
	EA
	
	

	159
	PGGC2Z103W07 4.000, Gasket, SpWnd, 825/Grph, 1/8", CL 150, B16.20, Gasket Incoloy 825 Flexible Graphite Filled ASME Class 150  S
	3
	EA
	
	

	160
	PGGC2S100609 6.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	10
	EA
	
	

	161
	PGGC1YJ00A09 6.000, Gasket, OvlRng, Soft Iron, R47, CL 2500, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  C
	34
	EA
	
	

	162
	PGGC2S300609 6.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled  A
	8
	EA
	
	

	163
	PGGC1YJ00A0A 8.000, Gasket, OvlRng, Soft Iron, R51, CL 2500, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  C
	55
	EA
	
	

	164
	PGGC2S10060A 8.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	7
	EA
	
	

	165
	PGGC2S10060B10.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	6
	EA
	
	

	166
	PGGC2S30060B10.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	32
	EA
	
	

	167
	PGGC1YJ00A0B10.000, Gasket, OvlRng, Soft Iron, R55, CL 2500, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  C
	17
	EA
	
	

	168
	PGGC2S10060C12.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	7
	EA
	
	

	169
	PGGC2S30060C12.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	15
	EA
	
	

	170
	PGGC2S10060D14.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL150, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	3
	EA
	
	

	171
	PGGC2S30060D14.000, Gasket, SpWnd, 316-FG, 1/8"SS, CL300, B16.20, B16.5, Gasket 316 Stainless Steel, Flexible Graphite Filled AS
	2
	EA
	
	

	172
	PGGC1Y600A0E16.000, Gasket, OvlRng, Soft Iron, R65, CL 600, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  Cl
	17
	EA
	
	

	173
	PGGC1Y600A0H24.000, Gasket, OvlRng, Soft Iron, R77, CL 600, B16.20, B16.5, Gasket Soft Iron, Max Brinell Hardness 90 HB ASME  Cl
	5
	EA
	
	

	174
	PGGC1Y60ZA0L30.000, Gasket, OvlRng, Soft Iron, R95, CL 600, B16.20, B16.47-A, Gasket, Soft Iron, Max Brinell Hardness 90HB ASME
	3
	EA
	
	

	 
	 
	 
	
	

	175
	FBBSFW000E0W16.00085.000, Bolt, StdBlt, A320B818MA, Stud Bolt - Threaded Full Length Stainless Steel Per ASTM A320 B8M Class 1
	10
	EA
	
	

	176
	FBBS7A000E2J24.000155.00, BOLT, StdBlt, 24mm X 155mm, A320L7M/7M, Stud Bolt – Threaded Full Length Alloy Steel Per ASTM A320-L
	160
	EA
	
	

	177
	FBBSFW000E2120.000155.00, Bolt, StdBlt, A320B818MA, Stud Bolt - Threaded Full Length Stainless Steel Per ASTM A320 B8M Class 1
	66
	EA
	
	

	178
	FBBSFW000E20 20.000175.000, Bolt, StdBlt, M20x175mm, A320B818MA, Stud Bolt - Threaded Full Length Stainless Steel Per ASTM A320
	14
	EA
	
	

	179
	FBBS7A000E3C27.000200.00, BOLT, StdBlt, 27mm X 200mm, A320L7M/7M, Stud Bolt – Threaded Full Length Alloy Steel Per ASTM A320-L
	66
	EA
	
	

	180
	FBBS7A000E3K27.000245.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	52
	EA
	
	

	181
	FBBS7A000ECZ52.000435.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	150
	EA
	
	

	182
	FBBS7A000ED252.000480.00, BOLT, StdBlt, 52mm X 480mm, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M
	400
	EA
	
	

	183
	FBBS7A000ED952.000525.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	44
	EA
	
	

	184
	FBBS7A000EMU52.000580.00, BOLT, StdBlt, 52mm X 580mm, A320L7M/7M, Stud Bolt – Threaded Full Length Alloy Steel Per ASTM A320-L
	140
	EA
	
	

	185
	FBBS7A000EA1 14.000 70.000, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Thread ed Full Length Alloy Steel Per ASTM A320-L7M with Two C
	18
	EA
	
	

	186
	14.000 75.000, BOLT, StdBlt, A320L7M/7M, with 2 A194-7M Nuts
	36
	EA
	
	

	187
	FBBS7A000E0W16.00085.000, BOLT, StdBlt, 16mm X 85mm A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M
	9
	EA
	
	

	188
	FBBS7A000E0X16.00090.000, BOLT, StdBlt, 16mm X 90mm A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M
	68
	EA
	
	

	189
	FBBS7A000E0Y16.000100.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	80
	EA
	
	

	190
	FBBS7A000E0Z16.000110.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	5
	EA
	
	

	191
	FBBS7A000E1R20.000115.00, BOLT, StdBlt, 20mm X 115mm A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM  A320-L7M
	44
	EA
	
	

	192
	FBBS7A000E1S20.000125.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	18
	EA
	
	

	193
	FBBS7A000E1U20.000135.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	9
	EA
	
	

	194
	FBBS7A000E1V20.000140.00, BOLT, StdBlt, 20mm X 140mm, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M
	16
	EA
	
	

	195
	FBBS7A000E2220.000185.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	35
	EA
	
	

	196
	FBBS7A000E2B24.000135.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	120
	EA
	
	

	197
	FBBS7A000E2J24.000155.00, BOLT, StdBlt, 24mm X 155mm, A320L7M/7M, Stud Bolt – Threaded Full Length Alloy Steel Per ASTM A320-L
	26
	EA
	
	

	198
	FBBS7A000E2F24.000160.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	14
	EA
	
	

	199
	FBBS7A000E3427.000150.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	26
	EA
	
	

	200
	FBBS7A000E3827.000175.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	360
	EA
	
	

	201
	FBBS7A000E3E27.000205.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	18
	EA
	
	

	202
	FBBS7A000EUQ 27.000265.000, BOLT, StdBlt, M27x265mm, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M
	52
	EA
	
	

	203
	30.000 X 285.00, BOLT, STDBLT, A320-L7M WITH 3 A194-7M NUTS
	52
	EA
	
	

	204
	FBBS7A000E3Y30.000190.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Two  Car
	120
	EA
	
	

	205
	FBBS7A000E3G 30.000 195.000, BOLT, StdBlt, M30x195mm, A320L7M/7M, Stud B olt - Threaded Full Length Alloy Steel Per ASTM A320-L7
	22
	EA
	
	

	206
	FBBS7A000E7C39.000320.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	200
	EA
	
	

	207
	FBBS7A000E7Q39.000395.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	66
	EA
	
	

	208
	FBBS7A000EBJ48.000410.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	100
	EA
	
	

	209
	FBBS7A000ECW52.000440.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three Ca
	60
	EA
	
	

	210
	FBBS7A000EFC64.000605.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	120
	EA
	
	

	211
	FBBS7A00ZB1R64.000735.00, BOLT, StdBlt, A320L7M/7M, Stud Bolt - Threaded Full Length Alloy Steel Per ASTM A320-L7M with Three  C
	40
	EA
	
	

	



