|  |  |
| --- | --- |
| Name and short description | Refrigerator, single-chamber, detached, volume 150-199 l, with freezer |
| Additional characteristic: | Fridge |
| amount | 8 |
| unit of measurement | Thing |
| Delivery conditions | DDP |
| Delivery address | KAZAKHSTAN, Mangistau region, Zhanaozen GA, Zhanaozen town, Mangistau region, Zhanaozen city |

Fridge Double chamber, Freezer location Top, Useful total volume, l 618, Number of doors 2, Number of cameras 2, Total number of boxes 2, Case material Metal, Control type Electronic, Compressor type Inverter, Number of compressors 1, Climatic class of refrigerator T ( from + 18 ° C to + 43 ° C), Nero efficiency class A +, Annual power consumption, kW / year 400, Refrigerant R600a, Noise level, dB 39, Convertible doors No, Open door signal No, LED lighting Yes, Useful volume x 457, Refrigeration system No frost, Number of shelves 3, Shelf material Tempered glass, Freezer, Freezer compartment, l 161, Freezer defrosting system No frost, Cooling capacity, kg per day 10, Autonomous storage freezer compartment, h 12, Number of sections 2, additional features Digital display Yes, Ice maker Yes, Dispenser Yes, Freshness zone No, Features Super-freeze mode, Rapid cooling, Dimensions Height, cm 186.2, Width and, 83.6 cm, depth 78.8 cm, Weight 99, Outer carton Gross Weight 105 "Note: The potential supplier in the technical documentation shall specify the country and the factory of the manufacturer of the delivered goods. Warranty period: 12 months from the date of commissioning, but not less than 24 months from the date of delivery